Here is UPS Manager help doc and comment(version and other).

/*==================English Readme==============================*/
1.Software  installation and operation
i) soft installation
	copy the package ups_manager to you favorite directory , example :/root/tmp
                 Use the tar command to extract files from the diskette or software package:  
                        tar -xvf  ups_manager.tar
                 Change the working directory to /tmp. 
                         cd /root/tmp
                 Execute the installation program:
                         ./install.sco.sh
                The installation program will not execute in some shell scripts. If this happens, change to another shell script and  try again.
                the installation program  will automatically copy files to the default location   "/etc/RichComm/ups_manager/" and modify the system startup file to contain the 
                ups_manager for UNIX daemon process. 
        ii) start program 
                The installation program        will automatically start the main program . 
                 you can start it use following command:
                        ./ups_manager start
        iii) stop program
                 you can start it use following command:
                ./ups_manager stop
        iv) config program
                 you can start it use following command:
                ./ups_manager config
2.software package 
./ups_monitor
./ups_status
./ups_config
./shutdown.sh
./ups_manager
./ups_manager start                            start monitoring software
./ups_manager stop                             stop monitoring software
./ups_manager config                           config monitoring software
./ups_manager status			       view status parameters
./ups_manager restart                          restart monitoring software
./TimeCfg.conf
./install.sco.sh
./Readme
./SendMSG.sh


3.contact us and technical support